Aether Help
Index

# Automatic ITU zone determination

Aether can automatically determine the ITU zone for a callsign when it is entered. With this feature enabled, As soon as you hit enter after entering a callsign into a QSO, Aether will automatically determine the ITU zone from the callsign prefix, and fill in the ITU zone field for the QSO. Follow the steps below to use this feature.

To enable automatic ITU zone lookup:

1. Open Aether preferences from the application menu
2. Select the pane titled "General"
3. Check the box next to "ITU Zone" under "Automatically Lookup:"

## See also

Automatically determine country
Using automatic callbook lookup
Automatically determine DXCC code
Automatically determine CQ Zone
Callbook Lookup Topics
Aether Preferences Topics