Aether Help
Index

# Automatic DXCC code determination

Aether can automatically determine the DXCC code for a callsign when it is entered. With this feature enabled, As soon as you hit enter after entering a callsign into a QSO, Aether will automatically determine the DXCC code from the prefix, and fill in the DXCC code field for the QSO. Follow the steps below to use this feature.

To enable automatic DXCC code lookup:

1. Open Aether preferences from the application menu
2. Select the pane titled "General"
3. Check the box next to "DXCC Code" under "Automatically Lookup:"

## See also

Automatically determine country
Using automatic callbook lookup
Automatically determine ITU Zone
Automatically determine CQ Zone
Callbook Lookup Topics
Aether Preferences Topics