Aether Help
Index

# Rig control doesn't work

Please try the following steps to solve a problem with rig control in Aether:

- Verify that you've enabled rig control in Aether preferences.
- Make sure you've selected the correct serial port and radio type.
- Verify that the baud rate selected in the rig control tab of Aether's preferences matches the baud rate configured on your radio.
- Make sure your rig is on and connected, then reinitialize rig control by unchecking the "Enable rig control" box, then rechecking it.
- With rig control enabled, and your rig connected and turned on, quit Aether then reopen it.

If these steps fail to resolve the problem, please contact Aether support at support@aetherlog.com.

## See also

Using Rig Control in Aether
Rig Control Topics