Aether Help
Index

# Distance and Beam Heading Display

Aether has the ability to calculate the distance and beam heading from your station location to a logged contact. If you have filled in your station latitude and longitude in the Station Info window, and latitude and longitude have been filled in for the selected QSO, Aether will calculate and display the distance and beam heading automatically. By default, distance is displayed in miles for U.S. users, and in kilometers for everyone else. The displayed units can be toggled between miles and kilometers by clicking on the distance display.

## See also

Distance and Beam Heading Topics